A picture containing graphical user interface

Description automatically generated **Octophonic System**

**Technical Specifications**

**Layout**

The octophonic sound diffusion system for ICSC2022 is an 8.1 system consisting of:

* 8 x Neumann KH120A
* 1 x Neumann KH750 sub

The eight main monitors are distributed in a regular octagon, with channel 1 being Front Left (-22.5º), and the rest of the channels 45º apart in clockwise direction: -22.5, 22.5, 67.5, 112.5, 157.5, 202.5, 247.5, 292.5 (0°: front).

Diagram

Description automatically generated with medium confidence